It is mentioned in section 3.3.2.1.1 that ADC readings could be quite different from expected due to input noise, which is inevitable. However, the effects of those unwanted fluctuations could first be reduced by the use of an analogue filter. Since noise signals are usually