In Arduino platform, all communications with a DS18B20 device could be handled via a OneWire library. Since the 1-wire protocol is not a built-in in of the platform, a library must be installed manually. This thesis makes use of the OneWire library recommended by [https://www.arduino.cc/reference/en/libraries/onewire/], which is available in the Library Manager of Arduino IDE.